**Wheels Up Landing Certification By Analysis of Regional Jet Aircraft**

Yong Chen [[1]](#footnote-1), Qi Li[[2]](#footnote-2), Xiaodong Zhu [[3]](#footnote-3), and Guangrong Zhu [[4]](#footnote-4),

*COMAC (Commercial Aircraft Corporation of China), Shanghai, China*

and

Frank Abdi[[5]](#footnote-5), Harsh Baid[[6]](#footnote-6), and Jerry Housner [[7]](#footnote-7)

*AlphaSTAR Corporation, Long Beach, California 90804*

In this paper a building block certification strategy is implemented on Regional Jet for Wheels-Up Landing drop test condition compliance with FAR/CCAR 25.994. Multi-scale progressive Failure Dynamic Analysis (MS-PFDA) is implemented on large scale structural models prepared to predict significant deformations, damage and fracture evolution subject to wheels up landing (WUL) scenario. MS-PFDA was validated for B737 drop test scenario with fuel, and luggage. A building block MS-PFDA simulation validation strategy compared FAA conducted B737 fuselage drop tests for the final shape change, acceleration of floor panel, and velocity versus time for two test conditions: a) With fuel tank deformation; and b) With luggage only deformation. Next ARJ21 fuselage and APU fuel lines including a global FEM of the aircraft and local FEM models of fuel line joints were simulated for wheels up landing on a paved runway to determine possibility of fuel leakage. A sink rate of 5ft/sec based on minimum FAA WUL requirement and 17 ft/sec based on FAA reference documents where FAA performed wheels up landing of a B720 at 17ft/sec was selected for the wheels up landing simulations. Simulation results at 5 ft/sec and six degree pitch angle concluded that: (1) The fairing stays intact; (2) Maximum plastic strain in the fuel line is below the failure strain limits and the fuel tank remains intact; (3) Flex Joints reaches axial, and rotation limits, without major deformation and load bearing capability of flex joints are based on Local Flex Joint FEA results; and (4) The work focused on passenger safety by meeting requirements for floor panel acceleration shock wave duration & distribution due to fuel line leakage. Designated Engineering Representatives (DER) verified no leakage based on local flex joint FE model, and CAAC accepted Type certification by analysis supported by Test.

1. Chief Designer of ARJ21, COMAC SADRI. [↑](#footnote-ref-1)
2. Senior Engineer, COMAC SADRI. [↑](#footnote-ref-2)
3. Senior Engineer, COMAC SADRI. [↑](#footnote-ref-3)
4. Deputy Chief Designer of ARJ21, COMAC SADRI. [↑](#footnote-ref-4)
5. CTO, Material and Structures, and AIAA Senior Member. [↑](#footnote-ref-5)
6. Research Scientist, Material and Structures. [↑](#footnote-ref-6)
7. Senior Scientist, Material and Structures. [↑](#footnote-ref-7)